    1/*

    2 * PWM_sf_data.c

    3 *

    4 * Code generation for model "PWM_sf".

    5 *

    6 * Model version              : 1.825

    7 * Simulink Coder version : 9.4 (R2020b) 29-Jul-2020

    8 * C source code generated on : Fri Apr 14 12:53:29 2023

    9 *

    10 * Target selection: rtwsfcn.tlc

    11 * Note: GRT includes extra infrastructure and instrumentation for prototyping

    12 * Embedded hardware selection: ARM Compatible->ARM Cortex-M

    13 * Emulation hardware selection:

    14 *    Differs from embedded hardware (MATLAB Host)

    15 * Code generation objectives:

    16 *    1. Execution efficiency

    17 *    2. RAM efficiency

    18 * Validation result: Not run

    19 */

    20

    21#include "PWM_sf.h"

    22#include "PWM_sf_private.h"

    23

    24/* Constant parameters (default storage) */

    25const ConstP_PWM_T PWM_ConstP = {

    26  /* Expression: rep_seq_y

    27   * Referenced by: '<S3>/Look-Up Table1'

    28   */

    29  { 0.0, 3000.0, 0.0 },

    30

    31  /* Expression: rep_seq_t - min(rep_seq_t)

    32   * Referenced by: '<S3>/Look-Up Table1'

    33   */

    34  { 0.0, 5.0E-5, 0.0001 }

    35};

    36