    1

    2

    3    /*

    4  * rtGetInf.h

    5  *

    6    * Code generation for model "PWM_sf".

    7  *

    8  * Model version              : 1.825

    9  * Simulink Coder version : 9.4 (R2020b) 29-Jul-2020

    10  * C source code generated on : Fri Apr 14 12:53:29 2023

    11 *

    12 * Target selection: rtwsfcn.tlc

    13 * Note: GRT includes extra infrastructure and instrumentation for prototyping

    14 * Embedded hardware selection: ARM Compatible->ARM Cortex-M

    15 * Emulation hardware selection:

    16 *    Differs from embedded hardware (MATLAB Host)

    17 * Code generation objectives:

    18 *    1. Execution efficiency

    19 *    2. RAM efficiency

    20 * Validation result: Not run

    21  */

    22

    23

    24  #ifndef RTW_HEADER_rtGetInf_h_

    25  #define RTW_HEADER_rtGetInf_h_

    26

    27

    28

    29

    30

    31#include <stddef.h>

    32  #include "rtwtypes.h"

    33  #include "rt_nonfinite.h"

    34

    35

    36

    37

    38

    39

    40

    41

    42

    43

    44

    45

    46

    47

    48

    49

    50

    51

    52

    53

    54

    55

    56

    57

    58

    59

    60

    61

    62

    63

    64

    65

    66    extern real_T rtGetInf(void);

    67      extern real32_T rtGetInfF(void);

    68      extern real_T rtGetMinusInf(void);

    69      extern real32_T rtGetMinusInfF(void);

    70

    71

    72

    73

    74

    75

    76

    77

    78

    79

    80

    81

    82

    83    #endif /* RTW_HEADER_rtGetInf_h_ */

    84