    1/*

    2 * PWM_sid.h

    3 *

    4 * Code generation for model "PWM_sf".

    5 *

    6 * Model version              : 1.825

    7 * Simulink Coder version : 9.4 (R2020b) 29-Jul-2020

    8 * C source code generated on : Fri Apr 14 12:53:29 2023

    9 *

    10 * Target selection: rtwsfcn.tlc

    11 * Note: GRT includes extra infrastructure and instrumentation for prototyping

    12 * Embedded hardware selection: ARM Compatible->ARM Cortex-M

    13 * Emulation hardware selection:

    14 *    Differs from embedded hardware (MATLAB Host)

    15 * Code generation objectives:

    16 *    1. Execution efficiency

    17 *    2. RAM efficiency

    18 * Validation result: Not run

    19 *

    20 * SOURCES: PWM_sf.c

    21 */

    22

    23/* statically allocated instance data for model: PWM */

    24{

    25  {

    26    /* Local SimStruct for the generated S-Function */

    27    static LocalS slS;

    28    LocalS *lS = &slS;

    29    ssSetUserData(rts, lS);

    30

    31    /* block I/O */

    32    {

    33      static B_PWM_T sfcnB;

    34      void *b = (real_T *) &sfcnB;

    35      ssSetLocalBlockIO(rts, b);

    36      (void) memset(b, 0,

    37                    sizeof(B_PWM_T));

    38    }

    39

    40    /* model checksums */

    41    ssSetChecksumVal(rts, 0, 1460315084U);

    42    ssSetChecksumVal(rts, 1, 1873271935U);

    43    ssSetChecksumVal(rts, 2, 11797905U);

    44    ssSetChecksumVal(rts, 3, 1909962613U);

    45  }

    46}

    47